* Design and implementation of an efficient runtime-level failure detection and propagation strategy for HPC and distributed systems.
* Detection of both node and process failures depends on heartbeats and timeouts.
* Reliable broadcast with a low-degree topology that scales with the number of nodes rather than the number of processes.
* Support multiple hybrid applications and programming models. (e.g. MPI and OpenSHMEM)